**SKATING RSC-CARBON**

RSC-­‐CARBON are high-­‐range roller-­‐ski skating. They are available in three different sizes. You will find in this document all informations you need to choose the most adapted to your level and what you are looking for.

|  |  |  |  |
| --- | --- | --- | --- |
| **RSC-­‐CARBON 610** | | | **Price :** |
|  | **Product specification :**  RSC-­‐CARBON are perfect for high-­‐level competition. Their low profile format allows you to feel as if skiing on snow. The carbon frame guarantees an unequalled lightness as well as a very good stiffness for a better energy transmission to the roller-­‐ski. Their highly resistant monoblock forks also ensure stable trajectories and important reduction of vibrations. Sold by pair with wheels and bindings. | | |
| **Technical characteristics :**  **Frame:** 100% carbon  **Weight** (one ski with wheels): 1150,75g (+ bindings :137,75)  **Length**: 2' 0" axle to axle (610mm)  **Forks**: Monoblocks, alloy Aluminium 7075  **Clearance frame-ground**: 1" 1/8 (29mm)  **Clearance skiboot-ground**: 2" 1/4 (57mm) (bindings Salomon), 2" 5/8 (66mm) (bindings  Rottefella)  **Wheels**: 3" 15/16 x 0" 15/16 (100x24mm); hardness (speed) to choose  **Bearings**: ABEC 9 Waterproof  **Bindings**: to choose | | | |
| **Wheels available** :  -­‐ USP Competition : 74-­‐50 slow (pink) ; 76-­‐50 slow (yellow) ; 78-­‐50 slow (orange) ; 80-­‐50 medium (green) ; medium 82-­‐50 (red) (price +40)  -­‐ USE : 76-­‐35 slow ; 76-­‐50 slow ; 82-­‐50 medium ; 89-­‐50 fast  *The first number indicates the hardness/resistance of wheels. The second one shows the rebound/elasticity of wheels. The combination of these two values gives the speed of the wheels (slow : 10-­‐35 km/h ;*  *medium : 15-­‐40 km/h ; fast : 15-­‐50 km/h)* | | **Bindings available** :  -Salomon SNS pilot Equipe Skate  -Salomon SNS Prolink Skate  -­‐ Salomon SNS Pilot Sport Skate  -­‐ Salomon SNS Pilot Carbon RS Skate (price +10)  -­‐ Salomon SNS Pilot Carbon RS2 Skate (price +10)  -­‐ Rottefella NNN Xcelerator  *Warning : Bindings Salomon are adaptable only with SNS standard skiboots, and Rottefella bindings are adaptable only with NNN standard skiboots.* | |

# [www.barnettsports.com](http://www.barnettsports.com/)

|  |  |  |  |
| --- | --- | --- | --- |
| **RSC-­‐CARBON 570** | | | **Price :** |
|  | **Product specification :**  RSC-­‐CARBON are perfect for high-­‐level competition. They were made rather for young people and for athletes skiing with technique rather than strength. Their low profile format allows you to feel as if skiing on snow. The carbon frame guarantees an unequalled lightness as a very good stiffness for a better energy transmission to the roller-­‐ski. The frame length and the highly resistant monoblock forks also ensure stable trajectories and important reduction of vibrations. Sold by pair with wheels and bindings. | | |
| **Technical characteristics :**  **Frame:** 100% carbon  **Weight** (one ski with wheels ): 1140,75g (+ bindings : 137,75g)  **Length**: 1' 10" 7/16 (570mm) axle to axle  **Forks**: Monoblocks, alloy Aluminium 7075  **Clearance frame-ground**: 1" 1/8 (29mm)  **Clearance skiboot-ground**: 2" 1/4 (57mm) (bindings Salomon), 2" 5/8 (66mm) (bindings Rottefella)  **Wheels**: 3" 15/16 x 0" 15/16 (100x24mm); hardness (speed) to choose  **Bearings**: ABEC 9 Waterproof  **Bindings**: to choose | | | |
| **Wheels available** :  -­‐ USP Competition : 74-­‐50 slow (pink) ; 76-­‐50 slow (yellow) ; 78-­‐50 slow (orange) ; 80-­‐50 medium (green) ; medium 82-­‐50 (red) (price +40)  -­‐ USE : 76-­‐35 slow ; 76-­‐50 slow ; 82-­‐50 medium ; 89-­‐50 fast  *The first number indicates the hardness/resistance of wheels. The second one shows the rebound/elasticity of wheels. The combination of these two values gives the speed of the wheels (slow : 10-­‐35 km/h ; medium : 15-­‐40 km/h ; fast : 15-­‐50 km/h)* | | **Bindings available** :  -Salomon SNS pilot Equipe Skate  -Salomon SNS Prolink Skate  -­‐ Salomon SNS Pilot Sport Skate  -­‐ Salomon SNS Pilot Carbon RS Skate (price +10)  -­‐ Salomon SNS Pilot Carbon RS2 Skate (price +10)  -­‐ Rottefella NNN Xcelerator  *Warning : Bindings Salomon are adaptable only with SNS standard skiboots, and Rottefella bindings are adaptable only with NNN standard skiboots.* | |

[*www.barnettsports.com*](http://www.barnettsports.com/)

|  |  |  |  |
| --- | --- | --- | --- |
| **RSC-­‐CARBON 530** | | | **Price :** |
|  | **Product specification :**  RSC-­‐CARBON are perfect for an introduction to roller-­‐ski and for high-­‐level competition. Their low profile format allows you to feel as if skiing on snow. The carbon frame guarantees an unequalled lightness as well as a very good stiffness for a better energy transmission to the roller-­‐ski. Their highly resistant monoblock forks also ensure stable trajectories and important reduction of vibrations. Sold by pair with wheels and bindings. | | |
| **Technical characteristics :**  **Frame:** 100% carbon  **Weight** (one ski with wheels ): 1132,75g (+ bindings : 137,75 g)  **Length**: 1' 8" 7/8 (530mm) axle to axle  **Forks**: Monoblocks, alloy Aluminium 7075  **Clearance frame-ground**: 1" 1/8 (29mm)  **Clearance skiboot-ground**: 2" 1/4 (57mm) (bindings Salomon), 2" 5/8 (66mm) (bindings Rottefella)  **Wheels**: 3" 15/16 x 0" 15/16 (100x24mm); hardness (speed) to choose  **Bearings**: ABEC 9 Waterproof  **Bindings**: to choose | | | |
| **Wheels available** :  -­‐ USP Competition : 74-­‐50 slow (pink) ; 76-­‐50 slow (yellow) ; 78-­‐50 slow (orange) ; 80-­‐50 medium (green) ; medium 82-­‐50 (red) (price +40)  -­‐ USE : 76-­‐35 slow ; 76-­‐50 slow ; 82-­‐50 medium ; 89-­‐50 fast  *The first number indicates the hardness/resistance of wheels. The second one shows the rebound/elasticity of wheels. The combination of these two values gives the speed of the wheels (slow : 10-­‐35 km/h ; medium : 15-­‐40 km/h ; fast : 15-­‐50 km/h)* | | **Bindings available** :  -Salomon SNS pilot Equipe Skate  -Salomon SNS ProlinkSkate  -­‐ Salomon SNS Pilot Sport Skate  -­‐ Salomon SNS Pilot Carbon RS Skate (price +10)  -­‐ Salomon SNS Pilot Carbon RS2 Skate (price +10)  -­‐ Rottefella NNN Xcelerator  *Warning : Bindings Salomon are adaptable only with SNS standard skiboots, and Rottefella bindings are adaptable only with NNN standard skiboots.* | |

[*www.barnettsports.com*](http://www.barnettsports.com/)